**OVERVIEW**

Trussville Gas and Water system currently samples for Lead and Copper on a reduced monitoring schedule of every three years as required by the Environmental Protection Agency (EPA) Lead and Copper Rule and Alabama Department of Environmental Management (ADEM) regulations 335-11-7-.06 and 335-11-7-.07.

Currently 30 (Tier 1) sample locations within the water system have been selected based on certain criteria set by ADEM and EPA regulations. Attached is a list of 30 (Tier 1) primary sites and 10 (Tier 1) alternate sites that will be used for collection of the samples.

Due to an increase in security measures, the sites listed within this collection area contain no homeowner names just addresses within the water system.